Calibration points for GE Haier gas meters:

|  |  |
| --- | --- |
| **TG10/4 Ritter Gas Flow Meter** | |
| **Flow Rate (Liters/Hour)** | **Totalized Flow (Liters)** |
| 4 |  |
| 250 |  |
| 450 | 850 |
| 1100 | 1840 |
| 1300 |  |
| Everything in yellow is a flow/total that we use |  |

Please note the totalization of the volume readings in column 2.